HDD MDVR Recording files name rules:

Such as: **H20190808-095851P1N2P0**.avi

**H**: Means the DVR used for oversea market;

**Date-Time**: format is: YYMMDD-hhmmss 20190808

**Video System**: PAL---P, NTSC---N

**Video resolution**: 1 means D1, 2 means HD1, 3 means CIF, there are also A, B,C

**Recording video type**: A means alarm recording file; N means normal recording file.

**Channel number**: 1 means CH1, 2 means CH2, 3 means CH3, 4 means CH4

**Frame Rate**: normally represent P, if can also be other letter

**0**: No meaning

So **H20190808-095851P1N2P0**.avi represent:

Recording in Sata1

**Date**: 2019-08-08

**H**: DVR used in oversea market

**Date&Time**: 20190808- 09:58:51

**P**: PAL video system

**1**: D1 resolution

**N**: normal recording file

**2**: CH2 video

**P0**: standard frame rate