
# Analog Intercom User Manual

1. **Analog intercom wiring**



6 Pin analog intercom





|  |  |
| --- | --- |
| Analog intercom port | MDVR 24PIN port |
| 1 | A-OUT |
| 4 | 12V |
| 3 | GND |
| 2 | A-IN |
|  |  |
|  |  |

Note: Under normal circumstances, the analog intercom interface can be directly connected to the 24PIN interface.


1. **Connect analog intercom**


Log in to the IVMS client and select Voice Intercom to open. Select device and start talk.





**Old Web**





**New Web**