**SMS Commands**

**Text format:** user name, password, your phone number, whether to send back to or not (1 or 0), command

+admin,888888,13713584340,1,RESET:20,3600 //Restart command

+admin,888888,13713584340,1,GETGPS // Get GPS command

DVR will restart after settings of parameters under SET are finished!

+admin,888888,13713584340,1,SETDEVNUM:66666 //Set Dev-No., MDVR will restart after the setting.

+admin,888888,13713584340,1,SETCENTERIP:192.168.8.69:8080 //Set server IP and Port, MDVR will restart after the setting. \*\*IP and port must be sent simultaneously. Otherwise “ERR ip” prompt will appear and the revision will not take effect.

Set 3G/4G parameters. MDVR will restart after the setting.

+admin,888888,13713584340,1,SET3G:[WCDMA,3gnet,\*99#,card,card,]

 [EVDO,ctnet,#777,card,card,]

 [TD-SCDMA,CMNET,\*99\*\*\*1#,card,card,]

 [FDD,3gnet,\*99#,card,card,]

 [TDD,cmnet,\*99#,card,card,]

 [EVDOLTE,ctnet,\*99\*\*\*1#,card,card,]

+admin,888888,13713584340,1,GETSTATE:[3G][HDD][VIDEOSTATUS][DEVNUM][VER][MCUVER][PARAM]

//Get the status of each parameter of the device

 [VIDEOSTATUS]show Analog:4 IPC:4 CH1-CH8 status 0 or status 1

+admin,888888,13713584340,1,GETSIM // Get SIM card information（Showed on Vehicle info interface）

+admin,888888,13713584340,1,SETSIM:013507550000 // Set SIM card Number, DVR will restart automatically

Return：set simnum：