# Audio pick-up

**Audio Pickup in Vehicle**


**Advantage：**

1.high sensitivity;

2.low noise;

3.low distortion;

4.small size



**Specifications：**

Voltage Input: 9～15 V

Power current: 5 mA～60 mA

Sensitivity: 200mA/ubar

Frequency: 500～10000 HZ

Max output Voltage: 2V-upp

